**SW Production Manager**

-----------------------------image--------------------------------

**Hardware Specification**

* Control Unit(provided)
* LCD Display (provided)
* Random light (provided)
* Proximity Sensor (provided)
* Data Cable (provided)

**Hardware Setup**

--------------Full Image of unit --------------

1. Connect component
2. Connect the sensor cable to port A of control unit.
3. Connect the Random light cable to port B of control unit.
4. Connect the control unit and LCD display using provided data cable.
5. Connect the 5V DC power supply to LCD display.
6. Connect the power cable to control unit.
7. Power on the Control unit and LCD display.
8. Run the WSPM Icon in desktop on the LCD Display.

Case 01.